
	Model 
	AR61030 

	Species 
	SCARA     

	Number of axes 
	4  

	Arm length
	600mm   

	Axis Specification
	
X Axis
	Arm Length
	200mm   

	
	
	Rotation Range
	±145° 

	
	Y Axis
	Arm Length
	400mm   

	
	
	Rotation Range
	±150°  

	
	Z Axis
	Route
	300mm  

	
	R Axis
	Rotation Range
	±360°  

	Highest Speed
	X Axis
	300°/s   

	
	Y Axis
	375°/s   

	
	X,Y Axis Synthesis
	6.5m/s    

	
	Z Axis
	1.4m/s 

	
	R Axis
	1000°/s 

	Standard Cycle Time
	0.39s 

	Repeat 
Positioning 
Accuracy
	X,Y Axis
	±0.003mm 

	
	Z Axis
	±0.02mm 

	
	R Axis
	±0.01° 

	Rated / Max Load 
	10KG/20KG  

	R Axis Allow Load Moment of Inertia(Rated/Max)
	0.1 KG/㎡ 

	
	0.5 KG/㎡  

	User Signal Line
	0.2²×16Lines,  
8 Output,6 Input  

	Users Pipe 
	φ6×2 Root   

	Limit Protection 
	1.Software Limit 
2.Mechanical Limit(X,Y,Z Axis)

	Weight
	43.5KG  



AR61030机器人运动空间，外形及安装尺寸（单位：mm）：
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图片模糊，请提供清晰的图片

特征与功能：
1. 标准循环时间为0.39S
2. 臂长600mm
3. 额定/最大负载：10/20KG
4. 适配控制系统QC400A/QC410，支持多种通讯方式：串口、网络、USB等
5. 节省空间，性能优良，易于操作和编程，精度可达±0.02mm 
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